# Assignment - 4

|  |  |
| --- | --- |
| Register  Number | 721219106034 |
| Team ID | PNT2022TMID31893 |

**Question-1:**

Write code and connections in wokwi for the ultrasonic sensor. Whenever the distance is less than 100 cms send an "alert" to the IBM cloud and display in the device recent events. Upload document

with wokwi share link and images of

IBM cloud

# Program:

#include <WiFi.h> #include <PubSubClient.h> WiFiClientwifiClient;

String data3;

#define ORG "v6wg8x"

#define DEVICE\_TYPE "nodeMcu" #define DEVICE\_ID "NodeMCU" #define TOKEN "123456789"

#define speed 0.034

#define led 14

void callback(char\* topic, byte\* playload, unsigned intpayloadLength);

char server[] = ORG

".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot- 2/evt/Data/fmt/json";

char topic[] = "iot-2/cmd/test/fmt/String"; char authMethod[] = "use-token-auth"; char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, callback , wifiClient);

void publishData();

constinttrigpin=5; constintechopin=18; String command; String data="";

long duration;

float dist;

void setup()

{

Serial.begin(115200); pinMode(led, OUTPUT); pinMode(trigpin, OUTPUT); pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

}

void loop() {

bool isNearby = dist< 100; digitalWrite(led, isNearby);

publishData(); delay(500);

if (!client.loop()) {

mqttConnect();

}

}

void wifiConnect() { Serial.print("Connecting to "); Serial.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6);

while (WiFi.status() != WL\_CONNECTED) { delay(500);

Serial.print(".");

}

Serial.print("WiFi connected, IP address: "); Serial.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) { Serial.print("Reconnecting MQTT client to "); Serial.println(server);

while (!client.connect(clientId, authMethod,

token)) { Serial.print(".");

delay(500);

}

initManagedDevice(); Serial.println();

}

}

void initManagedDevice() { if (client.subscribe(topic)) {

// Serial.println(client.subscribe(topic)); Serial.println("IBM subscribe to cmd OK");

} else {

Serial.println("subscribe to cmd FAILED");

}

}

void publishData()

{

digitalWrite(trigpin,LOW);

digitalWrite(trigpin,HIGH);

delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2; if(dist<100){

String payload = "{\"Normal Distance\":"; payload += dist;

payload += "}";

Serial.print("\n"); Serial.print("Sending payload: "); Serial.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

}

if(dist>101 &&dist<111){

String payload = "{\"Alert distance\":";

payload += dist;

payload += "}";

Serial.print("\n"); Serial.print("Sending payload: "); Serial.println(payload);

if(client.publish(publishTopic, (char\*) payload.c\_str())) {

Serial.println("Warning crosses 110cm -- it automaticaly of the loop"); digitalWrite(led,HIGH);

}else {

Serial.println("Publish FAILED");

}

}

}

void callback(char\* subscribeTopic, byte\* payload, unsigned intpayloadLength){

Serial.print("callback invoked for topic:");

Serial.println(subscribeTopic); for(inti=0; i<payloadLength; i++){ dist += (char)payload[i];

}

Serial.println("data:"+ data3); if(data3=="lighton"){ Serial.println(data3); digitalWrite(led,HIGH);

}

data3="";

}

# Output:







