**Team ID**: PNT2022TMID31893

**Develop a python script**

import paho.mqtt.client as mqtt  
for received data from server  
def on\_connect(data\_iot, user, events):  
  print(“connected with code” + str(events))  
data = mqtt.Client()  
Data.on\_connect = on\_connect  
Data.on\_message = on\_message  
data.loop\_forever()